route_id,direction_id,direction
30X,1,Inbound
L,1,Inbound
L,0,Outbound
FBUS,0,Outbound
FBUS,1,Inbound
SF,0,Outbound
SF,1,Inbound
29,0,Outbound
29,1,Inbound
714,0,Outbound
714,1,Inbound
14R,1,Inbound
14R,0,Outbound
18,0,Outbound
18,1,Inbound
19,0,Outbound
19,1,Inbound
90,1,Inbound
90,0,Outbound
1X,1,Inbound
1X,0,Outbound
23,1,Inbound
23,0,Outbound
24,1,Inbound
24,0,Outbound
25,1,Inbound
25,0,Outbound
27,1,Inbound
27,0,Outbound
28,0,Outbound
28,1,Inbound
12,1,Inbound
12,0,Outbound
14,1,Inbound
14,0,Outbound
2,0,Outbound
2,1,Inbound
22,1,Inbound
22,0,Outbound
33,1,Inbound
33,0,Outbound
36,1,Inbound
36,0,Outbound
38R,0,Outbound
38R,1,Inbound
43,0,Outbound
43,1,Inbound
44,0,Outbound
44,1,Inbound
45,0,Outbound
45,1,Inbound
49,0,Outbound
49,1,Inbound
31,1,Inbound
31,0,Outbound
5,0,Outbound
5,1,Inbound
30,0,Outbound
30,1,Inbound
35,0,Outbound
35,1,Inbound
37,0,Outbound
37,1,Inbound
58,0,Outbound
58,1,Inbound
38,0,Outbound
38,1,Inbound
39,1,Inbound
39,0,Outbound
48,0,Outbound
48,1,Inbound
56,1,Inbound
56,0,Outbound
57,0,Outbound
57,1,Inbound
5R,1,Inbound
5R,0,Outbound
1,0,Outbound
1,1,Inbound
54,1,Inbound
54,0,Outbound
55,0,Outbound
55,1,Inbound
6,0,Outbound
6,1,Inbound
67,0,Outbound
67,1,Inbound
LOWL,0,Outbound
LOWL,1,Inbound
NBUS,0,Outbound
NBUS,1,Inbound
15,1,Inbound
15,0,Outbound
7,1,Inbound
7,0,Outbound
9R,0,Outbound
9R,1,Inbound
8AX,1,Inbound
8AX,0,Outbound
8BX,0,Outbound
8BX,1,Inbound
J,0,Outbound
J,1,Inbound
CA,1,Inbound
CA,0,Outbound
K,1,Inbound
K,0,Outbound
91,0,Outbound
91,1,Inbound
KBUS,0,Outbound
KBUS,1,Inbound
F,0,Outbound
F,1,Inbound
M,1,Inbound
M,0,Outbound
N,0,Outbound
N,1,Inbound
66,1,Inbound
66,0,Outbound
8,0,Outbound
8,1,Inbound
PM,1,Inbound
PM,0,Outbound
T,1,South
T,0,North
TBUS,1,South
TBUS,0,North
52,0,Outbound
52,1,Inbound
9,1,Inbound
9,0,Outbound
NOWL,1,Inbound
NOWL,0,Outbound
PH,0,Outbound
PH,1,Inbound
28R,0,Outbound
28R,1,Inbound
